DOS/32A warning (9004): mouse initialization failed

                                     


    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
